{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"merged":[[0,0,0,7],[1,0,1,7],[3,0,32,0],[3,1,15,1],[15,2,15,6],[16,1,26,1],[26,2,26,7],[27,1,32,1],[32,2,32,6],[33,1,37,1],[40,1,41,3],[40,4,40,7],[41,4,41,7]]}
["汕职院团委、艺体系联合举办2021届音乐专业学生毕业汇报演出晚会设备租赁项目报价表"]
[]
["类别",null,"项目","参数","数量","单位","单价","小计"]
[null,"音响系统","全有源线阵音箱","①12寸线性阵列音箱单元组合:1*12\"MF NeoNeo原装英国进口钕磁单元Celestion/ 2*2.5\"HF Neo原装英国进口钕磁单元Celestion\n②频率响应:60Hz~17KHz (±3dB)\n③高频阻抗8欧,额定功率180W,最大功率360W,灵敏度 (1 W/m):115dB,最大额定声压:140dB peak,@1m\n④中频阻抗8欧,额定功率500W,最大功率1000W,灵敏度 (1 W/m):108dB,最大额定声压:135dB peak,@1m\n⑤扩散角(HXV):75°× 15°                                         \n⑦净重:24.5kg                                 \n⑧尺寸（长×宽×高）：582×414×343mm  ",8,"只"]
[null,null,"全有源超低音箱","①单18″超低频音箱（直射式远程超低）\n②单元类型： 1 X 18″\n③功率：800 W\n④阻抗： 4 Ohm\n⑤灵敏度：106dB\n⑥最大声压级：132dB\n⑦频响范围：35Hz – 250Hz\n⑧重量：95.0kg",4,"只"]
[null,null,"监听音箱","功率：370w\n声压级：131dB(连续);137dB(峰值)\n覆盖角度：100°(水平)×70°(垂直)\n外形尺寸H×W×D：436×628×445mm",2,"只"]
[null,null,"美国 JBL 音频处理器","2进6出",1,"台"]
[null,null,"无线麦克风","真分集 U频",8,"支"]
[null,null," FAMOUSOUND 功率放大器 ","8欧 1200W ",2,"台"]
[null,null,"英国 Soundcraft 调音台","S22 ",1,"台"]
[null,null,"联想笔记本",null,1,"台"]
[null,null,"电源线",null,1,"批"]
[null,null,"信号线",null,1,"批"]
[null,null,"调音师",null,null,"人"]
[null,null,"话筒助理师",null,null,"人"]
[]
[null,"灯光系统","DAGE BEAM光束电脑灯","额定总功率：450W，PFC功率因素补偿，功率波动（±50W）的环境下亦可正常使用。\n电压/频率：采用自主研发的AC90－260V/50-60HZ宽电压开关电源，可满足全球不同国家的电压和频率的要求。\n电源品质：采用高技术恒流电源板，所有PCB板元件均选用国内外一流品牌；AC专供电压模式，输出电压稳定、工作寿命长，抗干扰能力强。\n地线设置：按照国际地线接线的标准，更好提高安全性和稳定性。\n滤波保护：每台灯具，内置高品质的电源滤波器与磁环，隔离电网对灯具的干扰，保证灯具的稳定性。\n灯具线材：电源线防寒防冻，符合CE20/22标准，手拉手的设计。\n电源接口：配置二个电源接口，手拉手双电源模式。",16,"支"]
[null,null,"DAGE LED 4合一染色 PAR灯","额定功率：250W，功率相互补偿，波动（±50W）的环境下亦可正常使用。\n电压/频率：采用自主研发的AC100－260V/50-60HZ宽电压开关电源，可满足全球不同国家的电压和频率的要求。\n电源品质：采用高技术恒流电源板，所有PCB板元件均选用国内外一流品牌， AC专供电压模式，输出电压稳定、工作寿命长，抗干扰能力强。\n灯具线材：1.5米长的电源线和信号线材，防寒防冻，符合CE、GB7000.15-2000和CE20/CE22标准。",24,"支"]
[null,null," LED  PAR 聚光 面光灯","额定功率：250W，功率相互补偿，波动（±50W）的环境下亦可正常使用。\n电压/频率：采用自主研发的AC100－260V/50-60HZ宽电压开关电源，可满足全球不同国家的电压和频率的要求。\n电源品质：采用高技术恒流电源板，所有PCB板元件均选用国内外一流品牌， AC专供电压模式，输出电压稳定、工作寿命长，抗干扰能力强。\n灯具线材：1.5米长的电源线和信号线材，防寒防冻，符合CE、GB7000.15-2000和CE20/CE22标准。",8,"支"]
[null,null,"电源箱",null,1,"台"]
[null,null,"烟雾机",null,1,"台"]
[null,null,"金钢数码灯控台","DMX512/1990标准，最大1024个DMX控制通道，两路光电隔离信号输出。\n\n● 最大控制120台电脑灯或120路调光。\n\n● 新增ART-NET,内置模拟器功能\n\n\n● 新增RDM双向输出,可在控台设置灯的地址码\n\n● 使用珍珠灯库（R20格式灯库），且控台上可自行编写灯库。\n\n● 带背光的LCD显示屏，首创的中英文显示可切换界面。面板中英文可选。\n\n● 内置图形轨迹发生器，有227个内置图形，方便用户对电脑灯进行图形轨迹控制，如画圆、螺旋、彩虹、追逐等多种效果。\n\n● 图形参数（如：振幅、速度、间隔、波浪、方向）均可独立设置，更方便快捷的做出想要的造型和场景。\n\n● 每个场景可保存图形数量5个；同时可运行图形数量10个。\n\n● 有节目录制功能，最多可储存100个节目，灯光秀演示一劳永逸。",1,"台"]
[null,null,"电源线",null,1,"批"]
[null,null,"信号线",null,1,"批"]
[null,null,"电缆",null,1,"条"]
[null,null,"调光师、助理",null,null,"配套"]
[]
[null,"灯光架","400×400铝合金立柱 3米",null,6,"米"]
[null,null,"立柱底座",null,2,"套"]
[null,null,"三脚面光架",null,2,"套"]
[null,null,"螺丝工具",null,1,"项"]
[]
[]
[null,"LED屏","P3  LED显示屏","P3",24,"平米"]
[null,null,"迈普斯通V8+H8切换台控制器",null,1,"台"]
[null,null,"笔记本电脑(IBM T系列)",null,1,"台"]
[null,null,"线材",null,1,"项"]
[null,null,"垫高台","1米",1,"项"]
[null,"物料运输",null,null,1,"项"]
[null,"人工安装",null,null,1,"项"]
[{"$nulls":4},"                 总价：                            "]
[{"$nulls":4},"备注：报价中的所有价格应包含税费"]